BOREAS TF-08 NSA-OJP Tower Flux, Meteorological, and Soil Temperature Data



7.3 Data Characteristics



7.3.1 Parameter/Variable



The parameters contained in the data files are:



         Column Name

------------------------------

SITE_NAME

SUB_SITE

DATE_OBS

TIME_OBS

SENSIBLE_HEAT_FLUX_ABV_CNPY

LIC_LATENT_HEAT_FLUX_ABV_CNPY

LATENT_HEAT_FLUX_ABV_CNPY

NET_RAD_ABV_CNPY

CO2_FLUX_ABV_CNPY

DOWN_PPFD_ABV_CNPY

UP_PPFD_ABV_CNPY

WIND_SPEED_192CM

WIND_SPEED_635CM

WIND_SPEED_932CM

WIND_SPEED_1132CM

WIND_SPEED_1465CM

WIND_SPEED_ABV_CNPY

GILL_WIND_SPEED_ABV_CNPY

WIND_DIR_ABV_CNPY

FRICTION_VEL_ABV_CNPY

AIR_TEMP_ABV_CNPY

SOIL_HEAT_FLUX_CLOSED_102MM

SOIL_HEAT_FLUX_SEMI_CLOSE_64MM

SOIL_HEAT_FLUX_OPEN_64MM

SOIL_HEAT_FLUX_MOSS_40MM

SOIL_HEAT_FLUX_LICH_MOSS_40MM

SOIL_HEAT_FLUX_LICHEN_40MM

SOIL_TEMP_LICH_MOSS_25MM

SOIL_TEMP_LICH_MOSS_75MM

SOIL_TEMP_LICH_MOSS_200MM

SOIL_TEMP_MOSS_25MM

SOIL_TEMP_MOSS_100MM

SOIL_TEMP_MOSS_225MM

SOIL_TEMP_LICHEN_25MM

SOIL_TEMP_LICHEN_75MM

SOIL_TEMP_LICHEN_200MM

SOIL_TEMP_CLOSED_64MM

SOIL_TEMP_CLOSED_140MM

SOIL_TEMP_CLOSED_267MM

SOIL_TEMP_SEMI_CLOSED_25MM

SOIL_TEMP_SEMI_CLOSED_102MM

SOIL_TEMP_SEMI_CLOSED_229MM

SOIL_TEMP_OPEN_25MM

SOIL_TEMP_OPEN_102MM

SOIL_TEMP_OPEN_229MM

SOIL_WATER_POT_LICHEN_8CM

SOIL_WATER_POT_MOSS_8CM

RAINFALL_ABV_CNPY

RAINFALL_BELOW_CNPY

TROUGH_RAINFALL

DOWN_SOLAR_RAD_ABV_CNPY

UP_SOLAR_RAD_ABV_CNPY

AIR_TEMP_422CM

AIR_TEMP_932CM

AIR_TEMP_1565CM

SURF_PRESS

DOWN_LONGWAVE_RAD_ABV_CNPY

UP_LONGWAVE_RAD_ABV_CNPY

UP_LONGWAVE_RAD_SENSOR_TEMP

DOWN_LONGWAVE_RAD_SENSOR_TEMP

LONG_PLUS_SHORT_RAD_ABV_CNPY

SURF_TEMP_ABV_CNPY

SPECIFIC_HUM_422CM

SPECIFIC_HUM_932CM

SPECIFIC_HUM_1565CM

SPECIFIC_HUM_ABV_CNPY

REL_HUM_422CM

REL_HUM_932CM

REL_HUM_1565CM

REL_HUM_ABV_CNPY

SENSIBLE_HEAT_FLUX_BELOW_CNPY

LATENT_HEAT_FLUX_BELOW_CNPY

CO2_FLUX_BELOW_CNPY

NET_RAD_OPEN_100CM

NET_RAD_BELOW_CNPY

CRTFCN_CODE

REVISION_DATE



7.3.2 Variable Description/Definition



The descriptions of the parameters contained in the data files are:



         Column Name                             Description

------------------------------ ------------------------------------------------

SITE_NAME                      The identifier assigned to the site by BOREAS, in

                               the format SSS-TTT-CCCCC, where SSS identifies

                               the portion of the study area: NSA, SSA, REG, 

                               TRN, and TTT identifies the cover type for the 

                               site, 999 if unknown, and CCCCC is the identifier

                               for site, exactly what it means will vary with 

                               site type.

SUB_SITE                       The identifier assigned to the sub-site by BOREAS

                               in the format GGGGG-IIIII, where GGGGG is the

                               group associated with the sub-site instrument,

                               e.g. HYD06 or STAFF, and IIIII is the identifier

                               for sub-site, often this will refer to an 

                               instrument.

DATE_OBS                       The date on which the data were collected.

TIME_OBS                       The Greenwich Mean Time (GMT) of the start of the 
                               data collection.

SENSIBLE_HEAT_FLUX_ABV_CNPY    The sensible heat flux measured above the canopy.

LIC_LATENT_HEAT_FLUX_ABV_CNPY  The latent heat flux measured above the canopy 

                               using a Li-Cor instrument.

LATENT_HEAT_FLUX_ABV_CNPY      The latent heat flux measured above the canopy.

NET_RAD_ABV_CNPY               The net radiation measured above the canopy.

CO2_FLUX_ABV_CNPY              The carbon dioxide flux measured above the 

                               canopy.

DOWN_PPFD_ABV_CNPY             The downward (incoming) photosynthetic photon 

                               flux density measured above the canopy.

UP_PPFD_ABV_CNPY               The reflected photosynthetic photon flux density

                               measured above the canopy.

WIND_SPEED_192CM               The wind speed measured 1.92 m above the ground.

WIND_SPEED_635CM               The wind speed measured 6.35 m above the ground.

WIND_SPEED_932CM               The wind speed measured 9.32 m above the ground.

WIND_SPEED_1132CM              The wind speed measured 11.32 m above the ground.

WIND_SPEED_1465CM              The wind speed measured 14.65 m above the ground.

WIND_SPEED_ABV_CNPY            The wind speed measured above the canopy.  In 

                               this case at 18.88 m above the ground.

GILL_WIND_SPEED_ABV_CNPY       The wind speed measured above the canopy with the

                               Gill anemometer at 25.7 m above the ground.

WIND_DIR_ABV_CNPY              The direction from which the wind is blowing (in

                               creasing in a clockwise direction from the North)

                               and measured above the canopy at 25.7 m above the

                               ground.

FRICTION_VEL_ABV_CNPY          The friction velocity above the canopy.

AIR_TEMP_ABV_CNPY              The air temperature measured above the canopy.

SOIL_HEAT_FLUX_CLOSED_102MM    The soil heat flux measured at 10.16 cm depth at

                               a site under closed canopy.

SOIL_HEAT_FLUX_SEMI_CLOSE_64MM The soil heat flux measured at 6.35 cm depth at

                               a site under a semi-closed canopy.

SOIL_HEAT_FLUX_OPEN_64MM       The soil heat flux measured at 6.35 cm depth at

                               an open site.

SOIL_HEAT_FLUX_MOSS_40MM       The soil heat flux measured at 4 cm depth at a 

                               moss covered site.

SOIL_HEAT_FLUX_LICH_MOSS_40MM  The soil heat flux measured at 4 cm depth at a 

                               lichen and moss covered site.

SOIL_HEAT_FLUX_LICHEN_40MM     The soil heat flux measured at 4 cm depth at a 

                               lichen covered site.

SOIL_TEMP_LICH_MOSS_25MM       Soil temperature at 2.5 cm depth at a lichen and

                               moss covered site.

SOIL_TEMP_LICH_MOSS_75MM       Soil temperature at 7.5 cm depth at a lichen and

                               moss covered site.

SOIL_TEMP_LICH_MOSS_200MM      Soil temperature at 20 cm depth at a lichen and

                               moss covered site.

SOIL_TEMP_MOSS_25MM            Soil temperature at 2.5 cm depth at a moss 

                               Covered site.

SOIL_TEMP_MOSS_100MM           Soil temperature at 10 cm depth at a moss covered

                               site.

SOIL_TEMP_MOSS_225MM           Soil temperature at 22.5 cm depth at a moss 

                               covered site.

SOIL_TEMP_LICHEN_25MM          Soil temperature at 2.5 cm depth at a lichen 

                               covered site.

SOIL_TEMP_LICHEN_75MM          Soil temperature at 7.5 cm depth at a lichen 

                               covered site.

SOIL_TEMP_LICHEN_200MM         Soil temperature at 20 cm depth at a lichen 

                               covered site.

SOIL_TEMP_CLOSED_64MM          Soil temperature at 6.4 cm depth at a site under

                               closed canopy.

SOIL_TEMP_CLOSED_140MM         Soil temperature at 13.97 cm depth at a site 

                               under closed canopy.

SOIL_TEMP_CLOSED_267MM         Soil temperature at 26.67 cm depth at a site 

                               under closed canopy.

SOIL_TEMP_SEMI_CLOSED_25MM     Soil temperature at 2.54 cm depth at a site under

                               a semi-closed canopy.

SOIL_TEMP_SEMI_CLOSED_102MM    Soil temperature at 10.16 cm depth at a site 

                               under a semi-closed canopy.

SOIL_TEMP_SEMI_CLOSED_229MM    Soil temperature at 22.86 cm depth at a site 

                               under a semi-closed canopy.

SOIL_TEMP_OPEN_25MM            Soil temperature at 2.54 cm depth at an open 

                               site.

SOIL_TEMP_OPEN_102MM           Soil temperature at 10.16 cm depth at an open 

                               site.

SOIL_TEMP_OPEN_229MM           Soil temperature at 22.86 cm depth at an open 

                               site.

SOIL_WATER_POT_LICHEN_8CM      The soil water potential at 8 cm depth at a 

                               lichen covered site.

SOIL_WATER_POT_MOSS_8CM        The soil water potential at 8 cm depth at a moss

                               covered site.

RAINFALL_ABV_CNPY              The amount of rainfall measured above the canopy.

                               In 1994 the measurement is over a 30 minute 

                               period, in 1996 over an hour.

RAINFALL_BELOW_CNPY            The amount of rainfall measured below the canopy

                               in a clearing. In 1994 the measurement is over

                               a 30 minute period, in 1996 over an hour.

TROUGH_RAINFALL                The amount of rainfall measured in a trough below

                               the canopy, the trough area is 9 times the 

                               collection area of the other rain gauges.  In 

                               1994the measurement is over a 30 minute period, 

                               in 1996 over an hour.

DOWN_SOLAR_RAD_ABV_CNPY        The downward (incoming) solar radiation measured

                               above the canopy.

UP_SOLAR_RAD_ABV_CNPY          The reflected (outgoing) solar radiation measured

                               above the canopy.

AIR_TEMP_422CM                 The air temperature measured at 4.22 meters above

                               the ground.

AIR_TEMP_932CM                 The air temperature measured at 9.32 meters above

                               the ground.

AIR_TEMP_1565CM                The air temperature measured at 15.65 meters 

                               Above the ground.

SURF_PRESS                     The atmospheric pressure measured at the station.

DOWN_LONGWAVE_RAD_ABV_CNPY     The downward (incoming) longwave radiation measu

                               measured above the canopy.

UP_LONGWAVE_RAD_ABV_CNPY       The upward (outgoing) longwave radiation measured

                               above the canopy.

UP_LONGWAVE_RAD_SENSOR_TEMP    The temperature of the sensor measuring the 

                               upward longwave radiation.

DOWN_LONGWAVE_RAD_SENSOR_TEMP  The temperature of the sensor measuring the 

                               downward longwave radiation.

LONG_PLUS_SHORT_RAD_ABV_CNPY   The sum of the longwave and shortwave 

                               radiation measurements.

SURF_TEMP_ABV_CNPY             The surface radiation temperature measured from

                               above the canopy.

SPECIFIC_HUM_422CM             The specific humidity measured at 4.22 meters 

                               above the ground.

SPECIFIC_HUM_932CM             The specific humidity measured at 9.32 meters 

                               above the ground.

SPECIFIC_HUM_1565CM            The specific humidity measured at 15.65 meters 

                               above the ground.

SPECIFIC_HUM_ABV_CNPY          The specific humidity measured above the canopy.

REL_HUM_422CM                  The relative humidity measured at 4.22 meters 

                               above the ground.

REL_HUM_932CM                  The relative humidity measured at 9.32 meters 

                               above the ground.

REL_HUM_1565CM                 The relative humidity measured at 15.65 meters 

                               above the ground.

REL_HUM_ABV_CNPY               The relative humidity measured above the canopy.

SENSIBLE_HEAT_FLUX_BELOW_CNPY  The sensible heat flux measured below the canopy.

LATENT_HEAT_FLUX_BELOW_CNPY    The latent heat flux measured below the canopy.

CO2_FLUX_BELOW_CNPY            The carbon dioxide flux measured below the 

                               canopy.

NET_RAD_OPEN_100CM             The net radiation measured at 1 meter in canopy

                               opening.

NET_RAD_BELOW_CNPY             The net radiation measured below the canopy.

CRTFCN_CODE                    The BOREAS certification level of the data.  

                               Examples are CPI (Checked by PI), CGR (Certified 

                               by Group), PRE (Preliminary), and CPI-??? (CPI 

                               but questionable).

REVISION_DATE                  The most recent date when the information in the

                               referenced data base table record was revised.



7.3.3 Unit of Measurement



The measurement units for the parameters contained in the data files are:



         Column Name                                Units

------------------------------ ------------------------------------------------

SITE_NAME                      [none]

SUB_SITE                       [none]

DATE_OBS                       [DD-MON-YYYY]

TIME_OBS                       [HHMM GMT]

SENSIBLE_HEAT_FLUX_ABV_CNPY    [Watts][meter^-2]

LIC_LATENT_HEAT_FLUX_ABV_CNPY  [Watts][meter^-2]

LATENT_HEAT_FLUX_ABV_CNPY      [Watts][meter^-2]

NET_RAD_ABV_CNPY               [Watts][meter^-2]

CO2_FLUX_ABV_CNPY              [micromoles][meter^-2][second^-1]

DOWN_PPFD_ABV_CNPY             [micromoles][meter^-2][second^-1]

UP_PPFD_ABV_CNPY               [micromoles][meter^-2][second^-1]

WIND_SPEED_192CM               [meters][second^-1]

WIND_SPEED_635CM               [meters][second^-1]

WIND_SPEED_932CM               [meters][second^-1]

WIND_SPEED_1132CM              [meters][second^-1]

WIND_SPEED_1465CM              [meters][second^-1]

WIND_SPEED_ABV_CNPY            [meters][second^-1]

GILL_WIND_SPEED_ABV_CNPY       [meters][second^-1]

WIND_DIR_ABV_CNPY              [degrees]

FRICTION_VEL_ABV_CNPY          [meters][second^-1]

AIR_TEMP_ABV_CNPY              [degrees Celsius]

SOIL_HEAT_FLUX_CLOSED_102MM    [Watts][meter^-2]

SOIL_HEAT_FLUX_SEMI_CLOSE_64MM [Watts][meter^-2]

SOIL_HEAT_FLUX_OPEN_64MM       [Watts][meter^-2]

SOIL_HEAT_FLUX_MOSS_40MM       [Watts][meter^-2]

SOIL_HEAT_FLUX_LICH_MOSS_40MM  [Watts][meter^-2]

SOIL_HEAT_FLUX_LICHEN_40MM     [Watts][meter^-2]

SOIL_TEMP_LICH_MOSS_25MM       [degrees Celsius]

SOIL_TEMP_LICH_MOSS_75MM       [degrees Celsius]

SOIL_TEMP_LICH_MOSS_200MM      [degrees Celsius]

SOIL_TEMP_MOSS_25MM            [degrees Celsius]

SOIL_TEMP_MOSS_100MM           [degrees Celsius]

SOIL_TEMP_MOSS_225MM           [degrees Celsius]

SOIL_TEMP_LICHEN_25MM          [degrees Celsius]

SOIL_TEMP_LICHEN_75MM          [degrees Celsius]

SOIL_TEMP_LICHEN_200MM         [degrees Celsius]

SOIL_TEMP_CLOSED_64MM          [degrees Celsius]

SOIL_TEMP_CLOSED_140MM         [degrees Celsius]

SOIL_TEMP_CLOSED_267MM         [degrees Celsius]

SOIL_TEMP_SEMI_CLOSED_25MM     [degrees Celsius]

SOIL_TEMP_SEMI_CLOSED_102MM    [degrees Celsius]

SOIL_TEMP_SEMI_CLOSED_229MM    [degrees Celsius]

SOIL_TEMP_OPEN_25MM            [degrees Celsius]

SOIL_TEMP_OPEN_102MM           [degrees Celsius]

SOIL_TEMP_OPEN_229MM           [degrees Celsius]

SOIL_WATER_POT_LICHEN_8CM      [megaPascals]

SOIL_WATER_POT_MOSS_8CM        [megaPascals]

RAINFALL_ABV_CNPY              [millimeters]

RAINFALL_BELOW_CNPY            [millimeters]

TROUGH_RAINFALL                [millimeters]

DOWN_SOLAR_RAD_ABV_CNPY        [Watts][meter^-2]

UP_SOLAR_RAD_ABV_CNPY          [Watts][meter^-2]

AIR_TEMP_422CM                 [degrees Celsius]

AIR_TEMP_932CM                 [degrees Celsius]

AIR_TEMP_1565CM                [degrees Celsius]

SURF_PRESS                     [kiloPascals]

DOWN_LONGWAVE_RAD_ABV_CNPY     [Watts][meter^-2]

UP_LONGWAVE_RAD_ABV_CNPY       [Watts][meter^-2]

UP_LONGWAVE_RAD_SENSOR_TEMP    [degrees Celsius]

DOWN_LONGWAVE_RAD_SENSOR_TEMP  [degrees Celsius]

LONG_PLUS_SHORT_RAD_ABV_CNPY   [Watts][meter^-2]

SURF_TEMP_ABV_CNPY             [degrees Celsius]

SPECIFIC_HUM_422CM             [grams][kilogram^-1]

SPECIFIC_HUM_932CM             [grams][kilogram^-1]

SPECIFIC_HUM_1565CM            [grams][kilogram^-1]

SPECIFIC_HUM_ABV_CNPY          [grams][kilogram^-1]

REL_HUM_422CM                  [percent]

REL_HUM_932CM                  [percent]

REL_HUM_1565CM                 [percent]

REL_HUM_ABV_CNPY               [percent]

SENSIBLE_HEAT_FLUX_BELOW_CNPY  [Watts][meter^-2]

LATENT_HEAT_FLUX_BELOW_CNPY    [Watts][meter^-2]

CO2_FLUX_BELOW_CNPY            [micromoles][meters^-2][second^-1]

NET_RAD_OPEN_100CM             [Watts][meter^-2]

NET_RAD_BELOW_CNPY             [Watts][meter^-2]

CRTFCN_CODE                    [none]

REVISION_DATE                  [DD-MON-YYYY]



7.3.4 Data Source



The source of the parameter values contained in the data files are:



         Column Name                             Data Source

------------------------------ ------------------------------------------------

SITE_NAME                      [Assigned by BORIS.]

SUB_SITE                       [Assigned by BORIS.]

DATE_OBS                       [Supplied by Investigator.]

TIME_OBS                       [Supplied by Investigator.]

SENSIBLE_HEAT_FLUX_ABV_CNPY    [Sonic anemometer]

LIC_LATENT_HEAT_FLUX_ABV_CNPY  [Li-Cor Infrared Gas Analyzer]

LATENT_HEAT_FLUX_ABV_CNPY      [Campbell Scientific Krypton hygrometer]

NET_RAD_ABV_CNPY               [Net radiometer]

CO2_FLUX_ABV_CNPY              [Infrared Gas Analyzer]

DOWN_PPFD_ABV_CNPY             [quantum sensor]

UP_PPFD_ABV_CNPY               [quantum sensor]

WIND_SPEED_192CM               [Met-One cup anemometer]

WIND_SPEED_635CM               [Met-One cup anemometer]

WIND_SPEED_932CM               [Met-One cup anemometer]

WIND_SPEED_1132CM              [Met-One cup anemometer]

WIND_SPEED_1465CM              [Met-One cup anemometer]

WIND_SPEED_ABV_CNPY            [Met-One cup anemometer]

GILL_WIND_SPEED_ABV_CNPY       [Gill propeller-vane anemometer]

WIND_DIR_ABV_CNPY              [Gill propeller-vane anemometer]

FRICTION_VEL_ABV_CNPY          [Sonic anemometer]

AIR_TEMP_ABV_CNPY              [air temperature probe]

SOIL_HEAT_FLUX_CLOSED_102MM    [soil heat flux plate]

SOIL_HEAT_FLUX_SEMI_CLOSE_64MM [soil heat flux plate]

SOIL_HEAT_FLUX_OPEN_64MM       [soil heat flux plate]

SOIL_HEAT_FLUX_MOSS_40MM       [soil heat flux plate]

SOIL_HEAT_FLUX_LICH_MOSS_40MM  [soil heat flux plate]

SOIL_HEAT_FLUX_LICHEN_40MM     [soil heat flux plate]

SOIL_TEMP_LICH_MOSS_25MM       [soil temperature probe]

SOIL_TEMP_LICH_MOSS_75MM       [soil temperature probe]

SOIL_TEMP_LICH_MOSS_200MM      [soil temperature probe]

SOIL_TEMP_MOSS_25MM            [soil temperature probe]

SOIL_TEMP_MOSS_100MM           [soil temperature probe]

SOIL_TEMP_MOSS_225MM           [soil temperature probe]

SOIL_TEMP_LICHEN_25MM          [soil temperature probe]

SOIL_TEMP_LICHEN_75MM          [soil temperature probe]

SOIL_TEMP_LICHEN_200MM         [soil temperature probe]

SOIL_TEMP_CLOSED_64MM          [soil temperature probe]

SOIL_TEMP_CLOSED_140MM         [soil temperature probe]

SOIL_TEMP_CLOSED_267MM         [soil temperature probe]

SOIL_TEMP_SEMI_CLOSED_25MM     [soil temperature probe]

SOIL_TEMP_SEMI_CLOSED_102MM    [soil temperature probe]

SOIL_TEMP_SEMI_CLOSED_229MM    [soil temperature probe]

SOIL_TEMP_OPEN_25MM            [soil temperature probe]

SOIL_TEMP_OPEN_102MM           [soil temperature probe]

SOIL_TEMP_OPEN_229MM           [soil temperature probe]

SOIL_WATER_POT_LICHEN_8CM      [gypsum soil moisture block]

SOIL_WATER_POT_MOSS_8CM        [gypsum soil moisture block]

RAINFALL_ABV_CNPY              [Campbell Scientific rain gauge]

RAINFALL_BELOW_CNPY            [Campbell Scientific rain gauge]

TROUGH_RAINFALL                [MRI tipping bucket rain gauge]

DOWN_SOLAR_RAD_ABV_CNPY        [albedometer]

UP_SOLAR_RAD_ABV_CNPY          [albedometer]

AIR_TEMP_422CM                 [air temperature probe]

AIR_TEMP_932CM                 [air temperature probe]

AIR_TEMP_1565CM                [air temperature probe]

SURF_PRESS                     [barometer]

DOWN_LONGWAVE_RAD_ABV_CNPY     [pyrgeometer]

UP_LONGWAVE_RAD_ABV_CNPY       [pyrgeometer]

UP_LONGWAVE_RAD_SENSOR_TEMP    [thermopile]

DOWN_LONGWAVE_RAD_SENSOR_TEMP  [thermopile]

LONG_PLUS_SHORT_RAD_ABV_CNPY   [albedometer and pyrgeometer]

SURF_TEMP_ABV_CNPY             [IR thermometer]

SPECIFIC_HUM_422CM             [hygrometer]

SPECIFIC_HUM_932CM             [hygrometer]

SPECIFIC_HUM_1565CM            [hygrometer]

SPECIFIC_HUM_ABV_CNPY          [hygrometer]

REL_HUM_422CM                  [psychrometer]

REL_HUM_932CM                  [psychrometer]

REL_HUM_1565CM                 [psychrometer]

REL_HUM_ABV_CNPY               [psychrometer]

SENSIBLE_HEAT_FLUX_BELOW_CNPY  [Sonic anemometer]

LATENT_HEAT_FLUX_BELOW_CNPY    [Campbell Scientific Krypton hygrometer]

CO2_FLUX_BELOW_CNPY            [Sonic anemometer]

NET_RAD_OPEN_100CM             [Net radiometer]

NET_RAD_BELOW_CNPY             [Net radiometer]

CRTFCN_CODE                    [Assigned by BORIS.]

REVISION_DATE                  [Assigned by BORIS.]



7.3.5  Data Range



The following table gives information about the parameter values found in

the data files.



                     Minimum        Maximum        Missng  Unrel  Below   Data

                     Data           Data           Data    Data   Detect  Not

Column Name          Value          Value          Value   Value  Limit   Cllctd

--------------------------------------------------------------------------------

SITE_NAME            NSA-OJP-FLXTR  NSA-OJP-FLXTR  None    None   None    None

SUB_SITE             9TF08-FLX01    9TF08-FLX01    None    None   None    None

DATE_OBS             24-MAY-1994    12-NOV-1996    None    None   None    None

TIME_OBS             0              2330           None    None   None    None

SENSIBLE_HEAT_FLUX_  -124.74        997.44         -999    None   None    Blank

ABV_CNPY

LIC_LATENT_HEAT_FLUX_ -39.49        701.34         -999    None   None    Blank

ABV_CNPY

LATENT_HEAT_FLUX_ABV_ -117.83       544.18         -999    None   None    Blank

CNPY

NET_RAD_ABV_CNPY     -703.8         326.69         -999    None   None    Blank

CO2_FLUX_ABV_CNPY    -15            8.409          -999    None   None    Blank

DOWN_PPFD_ABV_CNPY   -1980          2360           None    None   None    Blank

UP_PPFD_ABV_CNPY     -1080          2410           None    None   None    Blank

WIND_SPEED_192CM     -15.07         155.73         -999    None   None    Blank

WIND_SPEED_635CM     -114.69        175.63         -999    None   None    Blank

WIND_SPEED_932CM     -92.58         191.22         -999    None   None    Blank

WIND_SPEED_1132CM    -14.86         184.76         -999    None   None    Blank

WIND_SPEED_1465CM    -115.91        44.97          -999    None   None    Blank

WIND_SPEED_ABV_CNPY  -122.6         24.04          -999    None   None    Blank

GILL_WIND_SPEED_ABV_ .03            7.19           -999    None   None    Blank

CNPY

WIND_DIR_ABV_CNPY    1.14           359.18         -999    None   None    Blank

FRICTION_VEL_ABV_    0              2.626          -999    None   None    Blank

CNPY

AIR_TEMP_ABV_CNPY    -18.02         40.8           -999    None   None    Blank

SOIL_HEAT_FLUX_      -35.99         13.5           None    None   None    Blank

CLOSED_102MM

SOIL_HEAT_FLUX_SEMI_ -70.7          19.8           None    None   None    Blank

CLOSE_64MM

SOIL_HEAT_FLUX_OPEN_ -95.45         19.98          None    None   None    Blank

64MM

SOIL_HEAT_FLUX_MOSS_ -4.723         40.637         -999    None   None    Blank

40MM

SOIL_HEAT_FLUX_LICH_ -516.282       108.18         -999    None   None    Blank

MOSS_40MM

SOIL_HEAT_FLUX_      -288.485       171.79         -999    None   None    Blank

LICHEN_40MM

SOIL_TEMP_LICH_MOSS_ 8.205          24.397         -999    None   None    Blank

25MM

SOIL_TEMP_LICH_MOSS_ 4.955          16.135         -999    None   None    Blank

75MM

SOIL_TEMP_LICH_MOSS_ 4.019          59.389         -999    None   None    Blank

200MM

SOIL_TEMP_MOSS_25MM  3.723          59.051         -999    None   None    Blank

SOIL_TEMP_MOSS_100MM 4.962          59.678         -999    None   None    Blank

SOIL_TEMP_MOSS_225MM 4.962          59.678         -999    None   None    Blank

SOIL_TEMP_LICHEN_    6.191          46.177         -999    None   None    Blank

25MM

SOIL_TEMP_LICHEN_    6.642          44.703         -999    None   None    Blank

75MM

SOIL_TEMP_LICHEN_    7.133          42.94          -999    None   None    Blank

200MM

SOIL_TEMP_CLOSED_    -1.25          20.06          -999    None   None    Blank

64MM

SOIL_TEMP_CLOSED_    -.03           15.96          -999    None   None    Blank

140MM

SOIL_TEMP_CLOSED_    .08            14.62          -999    None   None    Blank

267MM

SOIL_TEMP_SEMI_      -3.5           24.18          -999    None   None    Blank

CLOSED_25MM

SOIL_TEMP_SEMI_      -.77           16.97          -999    None   None    Blank

CLOSED_102MM

SOIL_TEMP_SEMI_      -15.59         17.35          -999    None   None    Blank

CLOSED_229MM

SOIL_TEMP_OPEN_25MM  -.74           20.8           -999    None   None    Blank

SOIL_TEMP_OPEN_102MM -.54           19             -999    None   None    Blank

SOIL_TEMP_OPEN_229MM .21            18.12          -999    None   None    Blank

SOIL_WATER_POT_      -2.4807        -.032          None    None   None    Blank

LICHEN_8CM

SOIL_WATER_POT_MOSS_ -2.3104        -.0301         None    None   None    Blank

8CM

RAINFALL_ABV_CNPY    0              4.5            None    None   None    Blank

RAINFALL_BELOW_CNPY  0              8.2            None    None   None    Blank

TROUGH_RAINFALL      0              43.44          None    None   None    Blank

DOWN_SOLAR_RAD_ABV_  -944.88        235.38         -999    None   None    Blank

CNPY

UP_SOLAR_RAD_ABV_    -471.38        804.16         -999    None   None    Blank

CNPY

AIR_TEMP_422CM       -18.06         40.8           -999    None   None    Blank

AIR_TEMP_932CM       -18.21         38.49          -999    None   None    Blank

AIR_TEMP_1565CM      -18.42         41.13          -999    None   None    Blank

SURF_PRESS           95.65          997            -999    None   None    Blank

DOWN_LONGWAVE_RAD_   -530.27        -15.87         -999    None   None    Blank

ABV_CNPY

UP_LONGWAVE_RAD_ABV_ -69.45         1158.79        None    None   None    Blank

CNPY

DOWN_LONGWAVE_RAD_   -1.94          35.31          None    None   None    Blank

SENSOR_TEMP

UP_LONGWAVE_RAD_     -1.81          35.62          None    None   None    Blank

SENSOR_TEMP

LONG_PLUS_SHORT_RAD_ -750.83        545.71         None    None   None    Blank

ABV_CNPY

SURF_TEMP_ABV_CNPY   -109.58        104.94         -999    None   None    Blank

SPECIFIC_HUM_422CM   -530.6         3528.7         -999    None   None    Blank

SPECIFIC_HUM_932CM   -511.74        51.16          -999    None   None    Blank

SPECIFIC_HUM_1565CM  -831.9         156.11         -999    None   None    Blank

SPECIFIC_HUM_ABV_    -482.14        49.54          -999    None   None    Blank

CNPY

REL_HUM_422CM        16             203            -999    None   None    Blank

REL_HUM_932CM        10.63          175            -999    None   None    Blank

REL_HUM_1565CM       -72            156            -999    None   None    Blank

REL_HUM_ABV_CNPY     13.88          156            -999    None   None    Blank

SENSIBLE_HEAT_FLUX_  -149.6         593.58         -999    None   None    Blank

BELOW_CNPY

LATENT_HEAT_FLUX_    -84.39         509.86         -999    None   None    Blank

BELOW_CNPY

CO2_FLUX_BELOW_CNPY  -.227          1.591          -999    None   None    Blank

NET_RAD_OPEN_100CM   -996.95        1903.82        -999    None   None    Blank

NET_RAD_BELOW_CNPY   -998.65        1600.33        -999    None   None    Blank

CRTFCN_CODE          CPI            CPI            None    None   None    None

REVISION_DATE        14-JUL-1999    17-AUG-1999    None    None   None    None

--------------------------------------------------------------------------------

Minimum Data Value -- The minimum value found in the column.

Maximum Data Value -- The maximum value found in the column.

Missng Data Value  -- The value that indicates missing data. This is used to

                      indicate that an attempt was made to determine the

                      parameter value, but the attempt was unsuccessful.

Unrel Data Value   -- The value that indicates unreliable data.  This is used

                      to indicate an attempt was made to determine the

                      parameter value, but the value was deemed to be

                      unreliable by the analysis personnel.

Below Detect Limit -- The value that indicates parameter values below the

                      instruments detection limits.  This is used to

                      indicate that an attempt was made to determine the

                      parameter value, but the analysis personnel determined

                      that the parameter value was below the detection

                      limit of the instrumentation.

Data Not Cllctd    -- This value indicates that no attempt was made to

                      determine the parameter value.  This usually

                      indicates that BORIS combined several similar but

                      not identical data sets into the same data base table

                      but this particular science team did not

                      measure that parameter.



Blank -- Indicates that blank spaces are used to denote that type of value.

N/A   -- Indicates that the value is not applicable to the respective column.

None  -- Indicates that no values of that sort were found in the column.

--------------------------------------------------------------------------------



7.4 Sample Data Record



SITE_NAME,SUB_SITE,DATE_OBS,TIME_OBS,SENSIBLE_HEAT_FLUX_ABV_CNPY,

LIC_LATENT_HEAT_FLUX_ABV_CNPY,LATENT_HEAT_FLUX_ABV_CNPY,NET_RAD_ABV_CNPY,

CO2_FLUX_ABV_CNPY,DOWN_PPFD_ABV_CNPY,UP_PPFD_ABV_CNPY,WIND_SPEED_192CM,

WIND_SPEED_635CM,WIND_SPEED_932CM,WIND_SPEED_1132CM,WIND_SPEED_1465CM,

WIND_SPEED_ABV_CNPY,GILL_WIND_SPEED_ABV_CNPY,WIND_DIR_ABV_CNPY,FRICTION_VEL_ABV_CNPY,

AIR_TEMP_ABV_CNPY,SOIL_HEAT_FLUX_CLOSED_102MM,SOIL_HEAT_FLUX_SEMI_CLOSE_64MM,

SOIL_HEAT_FLUX_OPEN_64MM,SOIL_HEAT_FLUX_MOSS_40MM,SOIL_HEAT_FLUX_LICH_MOSS_40MM,

SOIL_HEAT_FLUX_LICHEN_40MM,SOIL_TEMP_LICH_MOSS_25MM,SOIL_TEMP_LICH_MOSS_75MM,

SOIL_TEMP_LICH_MOSS_200MM,SOIL_TEMP_MOSS_25MM,SOIL_TEMP_MOSS_100MM,

SOIL_TEMP_MOSS_225MM,SOIL_TEMP_LICHEN_25MM,SOIL_TEMP_LICHEN_75MM,

SOIL_TEMP_LICHEN_200MM,SOIL_TEMP_CLOSED_64MM,SOIL_TEMP_CLOSED_140MM,

SOIL_TEMP_CLOSED_267MM,SOIL_TEMP_SEMI_CLOSED_25MM,SOIL_TEMP_SEMI_CLOSED_102MM,

SOIL_TEMP_SEMI_CLOSED_229MM,SOIL_TEMP_OPEN_25MM,SOIL_TEMP_OPEN_102MM,

SOIL_TEMP_OPEN_229MM,SOIL_WATER_POT_LICHEN_8CM,SOIL_WATER_POT_MOSS_8CM,

RAINFALL_ABV_CNPY,RAINFALL_BELOW_CNPY,TROUGH_RAINFALL,DOWN_SOLAR_RAD_ABV_CNPY,

UP_SOLAR_RAD_ABV_CNPY,AIR_TEMP_422CM,AIR_TEMP_932CM,AIR_TEMP_1565CM,SURF_PRESS,

DOWN_LONGWAVE_RAD_ABV_CNPY,UP_LONGWAVE_RAD_ABV_CNPY,DOWN_LONGWAVE_RAD_SENSOR_TEMP,

UP_LONGWAVE_RAD_SENSOR_TEMP,LONG_PLUS_SHORT_RAD_ABV_CNPY,SURF_TEMP_ABV_CNPY,

SPECIFIC_HUM_422CM,SPECIFIC_HUM_932CM,SPECIFIC_HUM_1565CM,SPECIFIC_HUM_ABV_CNPY,

REL_HUM_422CM,REL_HUM_932CM,REL_HUM_1565CM,REL_HUM_ABV_CNPY,

SENSIBLE_HEAT_FLUX_BELOW_CNPY,LATENT_HEAT_FLUX_BELOW_CNPY,CO2_FLUX_BELOW_CNPY,

NET_RAD_OPEN_100CM,NET_RAD_BELOW_CNPY,CRTFCN_CODE,REVISION_DATE

'NSA-OJP-FLXTR','9TF08-FLX01',24-MAY-1994,1930,197.81,-999.0,-999.0,,-999.0,

,,,,,,,,,,.007,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,,-999.0,-999.0,

,,,'CPI',14-JUL-1999

'NSA-OJP-FLXTR','9TF08-FLX01',24-MAY-1994,2000,353.75,-999.0,-999.0,-999.0,

-999.0,2360.0,2410.0,1.09,1.2,1.67,2.2,2.9,3.37,,,.007,15.1,,,,,,,,,,,,,,,,,

,,,,,,,,,,,,,-999.0,-999.0,16.05,15.64,15.32,-999.0,-999.0,1158.65,35.29,35.6,

163.7,104.93,-507.93,-491.14,-479.45,-462.6,42.0,42.0,42.0,41.0,-999.0,-999.0,

,-999.0,1600.33,'CPI',14-JUL-1999

