BOREAS TF-10 NSA-YJP Tower Flux, Meteorological, and Porometry Data

7.3 Data Characteristics

The data provided by the TF-10 team consist of both tower flux and porometry 
measurements.  The details of these two data sets are contained in the following 
sections.

7.3.1 Parameter/Variable

The parameters contained in the flux data files are:

         Column Name
------------------------------
SITE_NAME
SUB_SITE
DATE_OBS
TIME_OBS
SENSIBLE_HEAT_FLUX_ABV_CNPY
LATENT_HEAT_FLUX_ABV_CNPY
NET_RAD_ABV_CNPY
CO2_FLUX_ABV_CNPY
CO2_CONC_ABV_CNPY
CO2_STORAGE
CO2_FLUX_ABV_PLUS_STORAGE
NIGHT_CO2_FLUX_ABV_CNPY
DOWN_PPFD_ABV_CNPY
UP_PPFD_ABV_CNPY
WIND_SPEED_510CM
WIND_SPEED_517CM
WIND_SPEED_610CM
WIND_SPEED_710CM
WIND_SPEED_715CM
WIND_SPEED_770CM
WIND_SPEED_910CM
WIND_SPEED_ABV_CNPY
MEAN_WIND_DIR_MAG_ABV_CNPY
SDEV_WIND_DIR_MAG_ABV_CNPY
AIR_TEMP_ABV_CNPY
H2O_FLUX_ABV_CNPY
SOIL_HEAT_FLUX_NORTH_10CM
SOIL_HEAT_FLUX_WEST_10CM
SOIL_TEMP_NORTH_1CM
SOIL_TEMP_NORTH_5CM
SOIL_TEMP_NORTH_10CM
SOIL_TEMP_NORTH_25CM
SOIL_TEMP_NORTH_50CM
SOIL_TEMP_NORTH_75CM
SOIL_TEMP_WEST_1CM
SOIL_TEMP_WEST_5CM
SOIL_TEMP_WEST_10CM
SOIL_TEMP_WEST_25CM
SOIL_TEMP_WEST_50CM
SOIL_TEMP_WEST_75CM
SOIL_TEMP_WEST_100CM
RAINFALL
DOWN_SOLAR_RAD_ABV_CNPY
UP_SOLAR_RAD_ABV_CNPY
NET_SOLAR_RAD_ABV_CNPY
DOWN_TOTAL_RAD_ABV_CNPY
UP_TOTAL_RAD_ABV_CNPY
AIR_TEMP_510CM
AIR_TEMP_517CM
AIR_TEMP_610CM
AIR_TEMP_710CM
AIR_TEMP_715CM
AIR_TEMP_770CM
AIR_TEMP_910CM
WET_BULB_TEMP_510CM
WET_BULB_TEMP_517CM
WET_BULB_TEMP_610CM
WET_BULB_TEMP_710CM
WET_BULB_TEMP_715CM
WET_BULB_TEMP_770CM
WET_BULB_TEMP_910CM
WET_BULB_TEMP_ABV_CNPY
VAPOR_PRESS_510CM
VAPOR_PRESS_517CM
VAPOR_PRESS_610CM
VAPOR_PRESS_710CM
VAPOR_PRESS_715CM
VAPOR_PRESS_770CM
VAPOR_PRESS_910CM
VAPOR_PRESS_ABV_CNPY
SURF_PRESS
DOWN_LONGWAVE_RAD_ABV_CNPY
UP_LONGWAVE_RAD_ABV_CNPY
CORR_NET_RAD_ABV_CNPY
ALBEDO
CNPY_AIR_TEMP_160CM
CNPY_WET_BULB_TEMP_160CM
CNPY_VAPOR_PRESS_160CM
MEAN_SMALL_TREE_BIOMASS_TEMP
MEAN_MEDIUM_TREE_BIOMASS_TEMP
MEAN_LARGE_TREE_BIOMASS_TEMP
TOTAL_HEAT_STORAGE_NORTH
TOTAL_HEAT_STORAGE_WEST
MEAN_TOTAL_HEAT_STORAGE
BIO_HEAT_STORAGE_NORTH
BIO_HEAT_STORAGE_WEST
MEAN_BIO_HEAT_STORAGE
SENSIBLE_AIR_HEAT_STORAGE
LATENT_AIR_HEAT_STORAGE
SOIL_HEAT_STORAGE_NORTH_10CM
SOIL_HEAT_STORAGE_WEST_10CM
MEAN_SPECIFIC_HUM_ABV_CNPY
SDEV_SPECIFIC_HUM_ABV_CNPY
MEAN_W_WIND_SPEED_ABV_CNPY
SDEV_W_WIND_SPEED_ABV_CNPY
REL_HUM_ABV_CNPY
CRTFCN_CODE
REVISION_DATE

The parameters contained in the porometry data files are:

         Column Name
------------------------------
SITE_NAME
SUB_SITE
DATE_OBS
TIME_OBS
TREE_HT_CLASS
MEASUREMENT_HT_CLASS
STOMATAL_CONDUCT_H2O
CRTFCN_CODE
REVISION_DATE

7.3.2 Variable Description/Definition

The descriptions of the parameters contained in the flux data files are:

         Column Name                             Description
------------------------------ ------------------------------------------------
SITE_NAME                      The identifier assigned to the site by BOREAS, 
                               in the format SSS-TTT-CCCCC, where SSS identifies
                               the portion of the study area: NSA, SSA, REG, 
                               TRN, and TTT identifies the cover type for the 
                               site, 999 if unknown, and CCCCC is the identifier
                               for site, exactly what it means will vary with 
                               site type.
SUB_SITE                       The identifier assigned to the sub-site by BOREAS
                               in the format GGGGG-IIIII, where GGGGG is the
                               group associated with the sub-site instrument,
                               e.g. HYD06 or STAFF, and IIIII is the identifier
                               for sub-site, often this will refer to an 
                               instrument.
DATE_OBS                       The date on which the data were collected.
TIME_OBS                       The Greenwich Mean Time (GMT) when the data were
                               collected.
SENSIBLE_HEAT_FLUX_ABV_CNPY    The sensible heat flux measured above the canopy.
LATENT_HEAT_FLUX_ABV_CNPY      The latent heat flux measured above the canopy.
NET_RAD_ABV_CNPY               The net radiation measured above the canopy.
CO2_FLUX_ABV_CNPY              The carbon dioxide flux measured above the 
                               canopy.
CO2_CONC_ABV_CNPY              The carbon dioxide concentration measured above
                               the canopy.
CO2_STORAGE                    The storage term of carbon dioxide under the eddy
                               flux system.
CO2_FLUX_ABV_PLUS_STORAGE      The sum of the above canopy carbon dioxide flux
                               and the under flux instrument storage term.
NIGHT_CO2_FLUX_ABV_CNPY        The nighttime carbon dioxide flux estimated from
                               a model based on temperature.
DOWN_PPFD_ABV_CNPY             The downward (incoming) photosynthetic photon 
                               flux density measured above the canopy.
UP_PPFD_ABV_CNPY               The reflected photosynthetic photon flux density
                               measured above the canopy.
WIND_SPEED_510CM               The wind speed measured 5.1 m above the ground.
WIND_SPEED_517CM               The wind speed measured 5.17 m above the ground.
WIND_SPEED_610CM               The wind speed measured 6.1 m above the ground.
WIND_SPEED_710CM               The wind speed measured 7.1 m above the ground.
WIND_SPEED_715CM               The wind speed measured 7.15 m above the ground.
WIND_SPEED_770CM               The wind speed measured 7.7 m above the ground.
WIND_SPEED_910CM               The wind speed measured 9.1 m above the ground.
WIND_SPEED_ABV_CNPY            The wind speed measured above the canopy.
MEAN_WIND_DIR_MAG_ABV_CNPY     The average wind direction in relation to 
                               magnetic north, over 30 minutes measured above 
                               the canopy.
SDEV_WIND_DIR_MAG_ABV_CNPY     The standard deviation of the wind direction in 
                               relation to magnetic north, over 30 minutes 
                               measured above the canopy.
AIR_TEMP_ABV_CNPY              The air temperature measured above the canopy.
H2O_FLUX_ABV_CNPY              The water vapor flux measured above the canopy.
SOIL_HEAT_FLUX_NORTH_10CM      The soil heat flux measured 10 cm below the soil
                               surface at a location north of the flux tower.
SOIL_HEAT_FLUX_WEST_10CM       The soil heat flux measured 10 cm below the soil
                               surface at a location west of the flux tower.
SOIL_TEMP_NORTH_1CM            Soil temperature 1 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_NORTH_5CM            Soil temperature 5 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_NORTH_10CM           Soil temperature 10 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_NORTH_25CM           Soil temperature 25 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_NORTH_50CM           Soil temperature 50 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_NORTH_75CM           Soil temperature 75 cm below the soil surface at
                               a location north of the flux tower.
SOIL_TEMP_WEST_1CM             Soil temperature 1 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_5CM             Soil temperature 5 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_10CM            Soil temperature 10 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_25CM            Soil temperature 25 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_50CM            Soil temperature 50 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_75CM            Soil temperature 75 cm below the soil surface at
                               a location west of the flux tower.
SOIL_TEMP_WEST_100CM           Soil temperature 1 m below the soil surface at a
                               location west of the flux tower.
RAINFALL                       The amount of rainfall measured above the canopy
                               in the 30 minute period following the given time.
DOWN_SOLAR_RAD_ABV_CNPY        The downward (incoming) solar radiation measured
                               above the canopy.
UP_SOLAR_RAD_ABV_CNPY          The reflected (outgoing) solar radiation measured
                               above the canopy.
NET_SOLAR_RAD_ABV_CNPY         The net solar radiation measured above the 
                               canopy.
DOWN_TOTAL_RAD_ABV_CNPY        The total downward (incoming) radiation measured
                               above the canopy.
UP_TOTAL_RAD_ABV_CNPY          The total upward (outgoing) radiation measured 
                               above the canopy.
AIR_TEMP_510CM                 The air temperature measured at 5.1 meters above
                               the ground.
AIR_TEMP_517CM                 The air temperature measured at 5.17 meters above
                               the ground.
AIR_TEMP_610CM                 The air temperature measured at 6.1 meters above
                               the ground.
AIR_TEMP_710CM                 The air temperature measured at 7.1 meters above
                               the ground.
AIR_TEMP_715CM                 The air temperature measured at 7.15 meters above
                               the ground.
AIR_TEMP_770CM                 The air temperature measured at 7.7 meters above
                               the ground.
AIR_TEMP_910CM                 The air temperature measured at 9.1 meters above
                               the ground.
WET_BULB_TEMP_510CM            The wet bulb temperature measured at 5.1 meters
                               above the ground.
WET_BULB_TEMP_517CM            The wet bulb temperature measured at 5.17 meters
                               above the ground.
WET_BULB_TEMP_610CM            The wet bulb temperature measured at 6.1 meters
                               above the ground.
WET_BULB_TEMP_710CM            The wet bulb temperature measured at 7.1 meters
                               above the ground.
WET_BULB_TEMP_715CM            The wet bulb temperature measured at 7.15 meters
                               above the ground.
WET_BULB_TEMP_770CM            The wet bulb temperature measured at 7.7 meters
                               above the ground.
WET_BULB_TEMP_910CM            The wet bulb temperature measured at 9.1 meters
                               above the ground.
WET_BULB_TEMP_ABV_CNPY         The wet bulb temperature measured above the 
                               canopy.
VAPOR_PRESS_510CM              The vapor pressure measured at 5.1 meters above
                               the ground.
VAPOR_PRESS_517CM              The vapor pressure measured at 5.17 meters above
                               the ground.
VAPOR_PRESS_610CM              The vapor pressure measured at 6.1 meters above
                               the ground.
VAPOR_PRESS_710CM              The vapor pressure measured at 7.1 meters above
                               the ground.
VAPOR_PRESS_715CM              The vapor pressure measured at 7.15 meters above
                               the ground.
VAPOR_PRESS_770CM              The vapor pressure measured at 7.7 meters above
                               the ground.
VAPOR_PRESS_910CM              The vapor pressure measured at 9.1 meters above
                               the ground.
VAPOR_PRESS_ABV_CNPY           The vapor pressure measured above the canopy.
SURF_PRESS                     The atmospheric pressure measured at the station.
DOWN_LONGWAVE_RAD_ABV_CNPY     The downward (incoming) longwave radiation 
                               measured above the canopy.
UP_LONGWAVE_RAD_ABV_CNPY       The upward (outgoing) longwave radiation measured
                               above the canopy.
CORR_NET_RAD_ABV_CNPY          The corrected net radiation measured above the 
                               canopy, using equations developed by Hodges and 
                               Smith (1997).
ALBEDO                         Surface solar albedo.
CNPY_AIR_TEMP_160CM            The air temperature in the canopy measured at 
                               1.6 meters above the ground.
CNPY_WET_BULB_TEMP_160CM       The wet bulb temperature in the canopy measured
                               at 1.6 meters above the ground.
CNPY_VAPOR_PRESS_160CM         The vapor pressure in the canopy measured at 1.6
                               meters above the ground.
MEAN_SMALL_TREE_BIOMASS_TEMP   The temperature of tree biomass in small trees.
                               Measured using thermocouples embedded directly
                               into the boles, 1/3 of the way up the tree and 
                               1/3 of the radius into the boles.  Three trees 
                               under 1.5 m height were measured.
MEAN_MEDIUM_TREE_BIOMASS_TEMP  The temperature of tree biomass in medium trees.
                                Measured using thermocouples embedded directly
                               into the boles, 1/3 of the way up the tree and
                               1/3 of the radius into the boles.  Three trees 
                               over 2.5 m height were measured.
MEAN_LARGE_TREE_BIOMASS_TEMP   The temperature of tree biomass in large trees.
                               Measured using thermocouples embedded directly
                               into the boles, 1/3 of the way up the tree and 
                               1/3 of the radius into the boles.  Three trees 
                               over 5 m height were measured.
TOTAL_HEAT_STORAGE_NORTH       Total of minor heat storage terms including soil
                               heat flux, storage in soil above flux plate, 
                               storage in biomass, and sensible and latent heat 
                               storage in the air at a location north of the 
                               flux tower.
TOTAL_HEAT_STORAGE_WEST        Total of minor heat storage terms including soil
                               heat flux, storage in soil above flux plate, 
                               storage in biomass, and sensible and latent heat 
                               storage in the air at a location west of the flux
                               tower.
MEAN_TOTAL_HEAT_STORAGE        Average of the north and west site total heat 
                               storage values.
BIO_HEAT_STORAGE_NORTH         Biomass heat storage for a site north of the flux
                               tower.
BIO_HEAT_STORAGE_WEST          Biomass heat storage for a site west of the flux
                               tower.
MEAN_BIO_HEAT_STORAGE          Average of the north and west site biomass heat
                               storage values.
SENSIBLE_AIR_HEAT_STORAGE      Sensible heat storage in air column between the
                               surface and net pyrradiometer.
LATENT_AIR_HEAT_STORAGE        Latent heat storage in air column between the 
                               surface and net pyrradiometer.
SOIL_HEAT_STORAGE_NORTH_10CM   Heat storage in the 10 cm of soil above the heat
                               flux plate at a location north of the flux tower
SOIL_HEAT_STORAGE_WEST_10CM    Heat storage in the 10 cm of soil above the heat
                               flux plate at a location west of the flux tower
MEAN_SPECIFIC_HUM_ABV_CNPY     The 30 minute mean specific humidity measured 
                               above the canopy.
SDEV_SPECIFIC_HUM_ABV_CNPY     The 30 minute standard deviation of specific 
                               humidity measured above the canopy.
MEAN_W_WIND_SPEED_ABV_CNPY     The 30 minute mean of the vertical wind speed 
                               measured above the canopy.
SDEV_W_WIND_SPEED_ABV_CNPY     The 30 minute standard deviation of the vertical
                               wind speed measured above the canopy.
REL_HUM_ABV_CNPY               The relative humidity measured above the canopy.
CRTFCN_CODE                    The BOREAS certification level of the data.  
                               Examples are CPI (Checked by PI), CGR (Certified 
                               by Group), PRE (Preliminary), and CPI-??? (CPI 
                               but questionable).
REVISION_DATE                  The most recent date when the information in the
                               referenced data base table record was revised.

The descriptions of the parameters contained in the porometry data files are:

         Column Name                             Description
------------------------------ ------------------------------------------------
SITE_NAME                      The identifier assigned to the site by BOREAS, 
                               in the format SSS-TTT-CCCCC, where SSS identifies
                               the portion of the study area: NSA, SSA, REG, 
                               TRN, and TTT identifies the cover type for the 
                               site, 999 if unknown, and CCCCC is the identifier
                               for site, exactly what it means will vary with 
                               site type.
SUB_SITE                       The identifier assigned to the sub-site by BOREAS
                               in the format GGGGG-IIIII, where GGGGG is the
                               group associated with the sub-site instrument,
                               e.g. HYD06 or STAFF, and IIIII is the identifier
                               for sub-site, often this will refer to an 
                               instrument.
DATE_OBS                       The date on which the data were collected.
TIME_OBS                       The Greenwich Mean Time (GMT) when the data were
                               collected.
TREE_HT_CLASS                  The height class of the tree being measured.
MEASUREMENT_HT_CLASS           The height class in the tree where the 
                               measurement was made.
STOMATAL_CONDUCT_H2O           Stomatal conductance of water vapor.
CRTFCN_CODE                    The BOREAS certification level of the data.  
                               Examples are CPI (Checked by PI), CGR (Certified 
                               by Group), PRE (Preliminary), and CPI-??? (CPI 
                               but questionable).
REVISION_DATE                  The most recent date when the information in the
                               referenced data base table record was revised.

7.3.3 Unit of Measurement

The measurement units for the parameters contained in the flux data files are:

         Column Name                                Units
------------------------------ ------------------------------------------------
SITE_NAME                      [none]
SUB_SITE                       [none]
DATE_OBS                       [DD-MON-YYYY]
TIME_OBS                       [HHMM GMT]
SENSIBLE_HEAT_FLUX_ABV_CNPY    [Watts][meter^-2]
LATENT_HEAT_FLUX_ABV_CNPY      [Watts][meter^-2]
NET_RAD_ABV_CNPY               [Watts][meter^-2]
CO2_FLUX_ABV_CNPY              [micromoles][meter^-2][second^-1]
CO2_CONC_ABV_CNPY              [parts per million]
CO2_STORAGE                    [micromoles][meter^-2][second^-1]
CO2_FLUX_ABV_PLUS_STORAGE      [micromoles][meter^-2][second^-1]
NIGHT_CO2_FLUX_ABV_CNPY        [micromoles][meter^-2][second^-1]
DOWN_PPFD_ABV_CNPY             [micromoles][meter^-2][second^-1]
UP_PPFD_ABV_CNPY               [micromoles][meter^-2][second^-1]
WIND_SPEED_510CM               [meters][second^-1]
WIND_SPEED_517CM               [meters][second^-1]
WIND_SPEED_610CM               [meters][second^-1]
WIND_SPEED_710CM               [meters][second^-1]
WIND_SPEED_715CM               [meters][second^-1]
WIND_SPEED_770CM               [meters][second^-1]
WIND_SPEED_910CM               [meters][second^-1]
WIND_SPEED_ABV_CNPY            [meters][second^-1]
MEAN_WIND_DIR_MAG_ABV_CNPY     [degrees from magnetic north]
SDEV_WIND_DIR_MAG_ABV_CNPY     [degrees from magnetic north]
AIR_TEMP_ABV_CNPY              [degrees Celsius]
H2O_FLUX_ABV_CNPY              [millimoles][meter^-2][second^-1]
SOIL_HEAT_FLUX_NORTH_10CM      [Watts][meter^-2]
SOIL_HEAT_FLUX_WEST_10CM       [Watts][meter^-2]
SOIL_TEMP_NORTH_1CM            [degrees Celsius]
SOIL_TEMP_NORTH_5CM            [degrees Celsius]
SOIL_TEMP_NORTH_10CM           [degrees Celsius]
SOIL_TEMP_NORTH_25CM           [degrees Celsius]
SOIL_TEMP_NORTH_50CM           [degrees Celsius]
SOIL_TEMP_NORTH_75CM           [degrees Celsius]
SOIL_TEMP_WEST_1CM             [degrees Celsius]
SOIL_TEMP_WEST_5CM             [degrees Celsius]
SOIL_TEMP_WEST_10CM            [degrees Celsius]
SOIL_TEMP_WEST_25CM            [degrees Celsius]
SOIL_TEMP_WEST_50CM            [degrees Celsius]
SOIL_TEMP_WEST_75CM            [degrees Celsius]
SOIL_TEMP_WEST_100CM           [degrees Celsius]
RAINFALL                       [millimeters]
DOWN_SOLAR_RAD_ABV_CNPY        [Watts][meter^-2]
UP_SOLAR_RAD_ABV_CNPY          [Watts][meter^-2]
NET_SOLAR_RAD_ABV_CNPY         [Watts][meter^-2]
DOWN_TOTAL_RAD_ABV_CNPY        [Watts][meter^-2]
UP_TOTAL_RAD_ABV_CNPY          [Watts][meter^-2]
AIR_TEMP_510CM                 [degrees Celsius]
AIR_TEMP_517CM                 [degrees Celsius]
AIR_TEMP_610CM                 [degrees Celsius]
AIR_TEMP_710CM                 [degrees Celsius]
AIR_TEMP_715CM                 [degrees Celsius]
AIR_TEMP_770CM                 [degrees Celsius]
AIR_TEMP_910CM                 [degrees Celsius]
WET_BULB_TEMP_510CM            [degrees Celsius]
WET_BULB_TEMP_517CM            [degrees Celsius]
WET_BULB_TEMP_610CM            [degrees Celsius]
WET_BULB_TEMP_710CM            [degrees Celsius]
WET_BULB_TEMP_715CM            [degrees Celsius]
WET_BULB_TEMP_770CM            [degrees Celsius]
WET_BULB_TEMP_910CM            [degrees Celsius]
WET_BULB_TEMP_ABV_CNPY         [degrees Celsius]
VAPOR_PRESS_510CM              [kiloPascals]
VAPOR_PRESS_517CM              [kiloPascals]
VAPOR_PRESS_610CM              [kiloPascals]
VAPOR_PRESS_710CM              [kiloPascals]
VAPOR_PRESS_715CM              [kiloPascals]
VAPOR_PRESS_770CM              [kiloPascals]
VAPOR_PRESS_910CM              [kiloPascals]
VAPOR_PRESS_ABV_CNPY           [kiloPascals]
SURF_PRESS                     [kiloPascals]
DOWN_LONGWAVE_RAD_ABV_CNPY     [Watts][meter^-2]
UP_LONGWAVE_RAD_ABV_CNPY       [Watts][meter^-2]
CORR_NET_RAD_ABV_CNPY          [Watts][meter^-2]
ALBEDO                         [unitless]
CNPY_AIR_TEMP_160CM            [degrees Celsius]
CNPY_WET_BULB_TEMP_160CM       [degrees Celsius]
CNPY_VAPOR_PRESS_160CM         [kiloPascals]
MEAN_SMALL_TREE_BIOMASS_TEMP   [degrees Celsius]
MEAN_MEDIUM_TREE_BIOMASS_TEMP  [degrees Celsius]
MEAN_LARGE_TREE_BIOMASS_TEMP   [degrees Celsius]
TOTAL_HEAT_STORAGE_NORTH       [Watts][meter^-2]
TOTAL_HEAT_STORAGE_WEST        [Watts][meter^-2]
MEAN_TOTAL_HEAT_STORAGE        [Watts][meter^-2]
BIO_HEAT_STORAGE_NORTH         [Watts][meter^-2]
BIO_HEAT_STORAGE_WEST          [Watts][meter^-2]
MEAN_BIO_HEAT_STORAGE          [Watts][meter^-2]
SENSIBLE_AIR_HEAT_STORAGE      [Watts][meter^-2]
LATENT_AIR_HEAT_STORAGE        [Watts][meter^-2]
SOIL_HEAT_STORAGE_NORTH_10CM   [Watts][meter^-2]
SOIL_HEAT_STORAGE_WEST_10CM    [Watts][meter^-2]
MEAN_SPECIFIC_HUM_ABV_CNPY     [grams][kilogram^-1]
SDEV_SPECIFIC_HUM_ABV_CNPY     [grams][kilogram^-1]
MEAN_W_WIND_SPEED_ABV_CNPY     [meters][second^-1]
SDEV_W_WIND_SPEED_ABV_CNPY     [meters][second^-1]
REL_HUM_ABV_CNPY               [percent]
CRTFCN_CODE                    [none]
REVISION_DATE                  [DD-MON-YYYY]

The measurement units for the parameters contained in the porometry data files 
are:

         Column Name                                Units
------------------------------ ------------------------------------------------
SITE_NAME                      [none]
SUB_SITE                       [none]
DATE_OBS                       [DD-MON-YYYY]
TIME_OBS                       [HHMM GMT]
TREE_HT_CLASS                  [meters]
MEASUREMENT_HT_CLASS           [meters]
STOMATAL_CONDUCT_H2O           [millimeters H2O][second^-1]
CRTFCN_CODE                    [none]
REVISION_DATE                  [DD-MON-YYYY]

7.3.4 Data Source

The source of the parameter values contained in the flux data files are:

         Column Name                             Data Source
------------------------------ ------------------------------------------------
SITE_NAME                      [Assigned by BORIS.]
SUB_SITE                       [Assigned by BORIS.]
DATE_OBS                       [Supplied by Investigator.]
TIME_OBS                       [Supplied by Investigator.]
SENSIBLE_HEAT_FLUX_ABV_CNPY    [sonic anemometer and thermocouple]
LATENT_HEAT_FLUX_ABV_CNPY      [sonic anemometer and krypton hygrometer]
NET_RAD_ABV_CNPY               [net pyrradiometer]
CO2_FLUX_ABV_CNPY              [IRGA and sonic anemometer]
CO2_CONC_ABV_CNPY              [IRGA]]
CO2_STORAGE                    [IRGA and sonic anemometer]
CO2_FLUX_ABV_PLUS_STORAGE      [IRGA and sonic anemometer]
NIGHT_CO2_FLUX_ABV_CNPY        [Supplied by Investigator.]
DOWN_PPFD_ABV_CNPY             [quantum sensor]
UP_PPFD_ABV_CNPY               [quantum sensor]
WIND_SPEED_510CM               [anemometer]
WIND_SPEED_517CM               [anemometer]
WIND_SPEED_610CM               [anemometer]
WIND_SPEED_710CM               [anemometer]
WIND_SPEED_715CM               [anemometer]
WIND_SPEED_770CM               [anemometer]
WIND_SPEED_910CM               [anemometer]
WIND_SPEED_ABV_CNPY            [anemometer]
MEAN_WIND_DIR_MAG_ABV_CNPY     [wind vane]
SDEV_WIND_DIR_MAG_ABV_CNPY     [wind vane]
AIR_TEMP_ABV_CNPY              [thermocouple]
H2O_FLUX_ABV_CNPY              [sonic anemometer and krypton hygrometer]
SOIL_HEAT_FLUX_NORTH_10CM      [heat flux plate]
SOIL_HEAT_FLUX_WEST_10CM       [heat flux plate]
SOIL_TEMP_NORTH_1CM            [thermocouple]
SOIL_TEMP_NORTH_5CM            [thermocouple]
SOIL_TEMP_NORTH_10CM           [thermocouple]
SOIL_TEMP_NORTH_25CM           [thermocouple]
SOIL_TEMP_NORTH_50CM           [thermocouple]
SOIL_TEMP_NORTH_75CM           [thermocouple]
SOIL_TEMP_WEST_1CM             [thermocouple]
SOIL_TEMP_WEST_5CM             [thermocouple]
SOIL_TEMP_WEST_10CM            [thermocouple]
SOIL_TEMP_WEST_25CM            [thermocouple]
SOIL_TEMP_WEST_50CM            [thermocouple]
SOIL_TEMP_WEST_75CM            [thermocouple]
SOIL_TEMP_WEST_100CM           [thermocouple]
RAINFALL                       [tipping bucket gauge]
DOWN_SOLAR_RAD_ABV_CNPY        [pyranometer]
UP_SOLAR_RAD_ABV_CNPY          [pyranometer]
NET_SOLAR_RAD_ABV_CNPY         [Supplied by Investigator.]
DOWN_TOTAL_RAD_ABV_CNPY        [Supplied by Investigator.]
UP_TOTAL_RAD_ABV_CNPY          [Supplied by Investigator.]
AIR_TEMP_510CM                 [thermocouple]
AIR_TEMP_517CM                 [thermocouple]
AIR_TEMP_610CM                 [thermocouple]
AIR_TEMP_710CM                 [thermocouple]
AIR_TEMP_715CM                 [thermocouple]
AIR_TEMP_770CM                 [thermocouple]
AIR_TEMP_910CM                 [thermocouple]
WET_BULB_TEMP_510CM            [thermocouple]
WET_BULB_TEMP_517CM            [thermocouple]
WET_BULB_TEMP_610CM            [thermocouple]
WET_BULB_TEMP_710CM            [thermocouple]
WET_BULB_TEMP_715CM            [thermocouple]
WET_BULB_TEMP_770CM            [thermocouple]
WET_BULB_TEMP_910CM            [thermocouple]
WET_BULB_TEMP_ABV_CNPY         [thermocouple]
VAPOR_PRESS_510CM              [temperature/relative humidity sensor]
VAPOR_PRESS_517CM              [temperature/relative humidity sensor]
VAPOR_PRESS_610CM              [temperature/relative humidity sensor]
VAPOR_PRESS_710CM              [temperature/relative humidity sensor]
VAPOR_PRESS_715CM              [temperature/relative humidity sensor]
VAPOR_PRESS_770CM              [temperature/relative humidity sensor]
VAPOR_PRESS_910CM              [temperature/relative humidity sensor]
VAPOR_PRESS_ABV_CNPY           [temperature/relative humidity sensor]
SURF_PRESS                     [pressure sensor]
DOWN_LONGWAVE_RAD_ABV_CNPY     [pyrgeometer]
UP_LONGWAVE_RAD_ABV_CNPY       [pyrgeometer]
CORR_NET_RAD_ABV_CNPY          [Supplied by Investigator.]
ALBEDO                         [Supplied by Investigator.]
CNPY_AIR_TEMP_160CM            [thermocouple]
CNPY_WET_BULB_TEMP_160CM       [thermocouple]
CNPY_VAPOR_PRESS_160CM         [temperature/relative humidity sensor]
MEAN_SMALL_TREE_BIOMASS_TEMP   [thermocouple]
MEAN_MEDIUM_TREE_BIOMASS_TEMP  [thermocouple]
MEAN_LARGE_TREE_BIOMASS_TEMP   [thermocouple]
TOTAL_HEAT_STORAGE_NORTH       [Supplied by Investigator.]
TOTAL_HEAT_STORAGE_WEST        [Supplied by Investigator.]
MEAN_TOTAL_HEAT_STORAGE        [Supplied by Investigator.]
BIO_HEAT_STORAGE_NORTH         [Supplied by Investigator.]
BIO_HEAT_STORAGE_WEST          [Supplied by Investigator.]
MEAN_BIO_HEAT_STORAGE          [Supplied by Investigator.]
SENSIBLE_AIR_HEAT_STORAGE      [Supplied by Investigator.]
LATENT_AIR_HEAT_STORAGE        [Supplied by Investigator.]
SOIL_HEAT_STORAGE_NORTH_10CM   [Supplied by Investigator.]
SOIL_HEAT_STORAGE_WEST_10CM    [Supplied by Investigator.]
MEAN_SPECIFIC_HUM_ABV_CNPY     [krypton hygrometer]
SDEV_SPECIFIC_HUM_ABV_CNPY     [krypton hygrometer]
MEAN_W_WIND_SPEED_ABV_CNPY     [sonic anemometer]
SDEV_W_WIND_SPEED_ABV_CNPY     [sonic anemometer]
REL_HUM_ABV_CNPY               [temperature/relative humidity sensor]
CRTFCN_CODE                    [Assigned by BORIS.]
REVISION_DATE                  [Assigned by BORIS.]

The source of the parameter values contained in the porometry data files are:

         Column Name                             Data Source
------------------------------ ------------------------------------------------
SITE_NAME                      [Assigned by BORIS.]
SUB_SITE                       [Assigned by BORIS.]
DATE_OBS                       [Supplied by Investigator.]
TIME_OBS                       [Supplied by Investigator.]
TREE_HT_CLASS                  [Supplied by Investigator.]
MEASUREMENT_HT_CLASS           [Supplied by Investigator.]
STOMATAL_CONDUCT_H2O           [Porometer]
CRTFCN_CODE                    [Assigned by BORIS.]
REVISION_DATE                  [Assigned by BORIS.]

7.3.5  Data Range

The following table gives information about the parameter values found in
the flux data files.

                     Minimum        Maximum        Missng  Unrel  Below   Data
                     Data           Data           Data    Data   Detect  Not
Column Name          Value          Value          Value   Value  Limit   Cllctd
--------------------------------------------------------------------------------
SITE_NAME            NSA-YJP-FLXTR  NSA-YJP-FLXTR  None    None   None    None
SUB_SITE             9TF10-FLX01    9TF10-FLX01    None    None   None    None
DATE_OBS             15-AUG-1993    09-NOV-1996    None    None   None    None
TIME_OBS             0              2330           None    None   None    None
SENSIBLE_HEAT_FLUX_  -69.59         458.28         -999    None   None    None
ABV_CNPY
LATENT_HEAT_FLUX_ABV -68.9          428.3          -999    None   None    None
_CNPY
NET_RAD_ABV_CNPY     -90.5          787            -999    None   None    None
CO2_FLUX_ABV_CNPY    -16.1          32.757         -999    None   None    Blank
CO2_CONC_ABV_CNPY    288.4          435.3          -999    None   None    Blank
CO2_STORAGE          -5.814         7.23           -999    None   None    Blank
CO2_FLUX_ABV_PLUS_   -16.09         10.494         -999    None   None    Blank
STORAGE
NIGHT_CO2_FLUX_ABV_  -2.619         5.748          -999    None   None    Blank
CNPY
DOWN_PPFD_ABV_CNPY   0              2100           -999    None   None    None
UP_PPFD_ABV_CNPY     0              360            -999    None   None    None
WIND_SPEED_510CM     .199           5.168          -999    None   None    Blank
WIND_SPEED_517CM     .199           6.223          -999    None   None    Blank
WIND_SPEED_610CM     .199           6.848          -999    None   None    Blank
WIND_SPEED_710CM     .199           6.022          -999    None   None    Blank
WIND_SPEED_715CM     .199           7.3            -999    None   None    Blank
WIND_SPEED_770CM     .199           7.59           -999    None   None    Blank
WIND_SPEED_910CM     .199           6.547          -999    None   None    Blank
WIND_SPEED_ABV_CNPY  .197           8.32           -999    None   None    None
MEAN_WIND_DIR_MAG_   0              359.9          -999    None   None    None
ABV_CNPY
SDEV_WIND_DIR_MAG_   0              78.1           -999    None   None    None
ABV_CNPY
AIR_TEMP_ABV_CNPY    -17.28         30.11          -999    None   None    None
H2O_FLUX_ABV_CNPY    -1.5283        7.8144         -999    None   None    None
SOIL_HEAT_FLUX_NORTH -31.4          73             -999    None   None    None
_10CM
SOIL_HEAT_FLUX_WEST_ -45.2          93.1           -999    None   None    None
10CM
SOIL_TEMP_NORTH_1CM  -1.86          31.61          -999    None   None    None
SOIL_TEMP_NORTH_5CM  -.44           24.64          -999    None   None    None
SOIL_TEMP_NORTH_10CM -.65           20.99          -999    None   None    None
SOIL_TEMP_NORTH_25CM -.66           17.66          -999    None   None    Blank
SOIL_TEMP_NORTH_50CM -.7            15.1           -999    None   None    Blank
SOIL_TEMP_NORTH_75CM -.65           13.26          -999    None   None    Blank
SOIL_TEMP_WEST_1CM   -2.9           34.43          -999    None   None    None
SOIL_TEMP_WEST_5CM   -.08           24.65          -999    None   None    None
SOIL_TEMP_WEST_10CM  -.15           19.55          -999    None   None    None
SOIL_TEMP_WEST_25CM  -.13           16.19          -999    None   None    None
SOIL_TEMP_WEST_50CM  -.2            13.87          -999    None   None    None
SOIL_TEMP_WEST_75CM  -.3            12.2           -999    None   None    None
SOIL_TEMP_WEST_100CM -.24           10.89          -999    None   None    None
RAINFALL             0              6.35           -999    None   None    None
DOWN_SOLAR_RAD_ABV_  0              1021           -999    None   None    None
CNPY
UP_SOLAR_RAD_ABV_    0              188.2          -999    None   None    None
CNPY
NET_SOLAR_RAD_ABV_   0              891.4          -999    None   None    None
CNPY
DOWN_TOTAL_RAD_ABV_  179.45         1365.5         -999    None   None    None
CNPY
UP_TOTAL_RAD_ABV_    229.8          632.9          -999    None   None    None
CNPY
AIR_TEMP_510CM       .373           26.8           -999    None   None    Blank
AIR_TEMP_517CM       -17.43         30.4           -999    None   None    Blank
AIR_TEMP_610CM       -.013          30.18          -999    None   None    Blank
AIR_TEMP_710CM       2.581          26.57          -999    None   None    Blank
AIR_TEMP_715CM       .156           29.45          -999    None   None    Blank
AIR_TEMP_770CM       -17.36         30.14          -999    None   None    Blank
AIR_TEMP_910CM       3.752          26.37          -999    None   None    Blank
WET_BULB_TEMP_510CM  .11            18.95          -999    None   None    Blank
WET_BULB_TEMP_517CM  -.136          19             -999    None   None    Blank
WET_BULB_TEMP_610CM  -.043          18.95          -999    None   None    Blank
WET_BULB_TEMP_710CM  3.641          18.78          -999    None   None    Blank
WET_BULB_TEMP_715CM  .077           18.95          -999    None   None    Blank
WET_BULB_TEMP_770CM  .132           18.94          -999    None   None    Blank
WET_BULB_TEMP_910CM  2.959          18.77          -999    None   None    Blank
WET_BULB_TEMP_ABV_   .156           18.92          -999    None   None    Blank
CNPY
VAPOR_PRESS_510CM    .5983          1.9357         -999    None   None    Blank
VAPOR_PRESS_517CM    .4654          1.9731         -999    None   None    Blank
VAPOR_PRESS_610CM    .4854          1.9724         -999    None   None    Blank
VAPOR_PRESS_710CM    .5872          1.9041         -999    None   None    Blank
VAPOR_PRESS_715CM    .4602          1.9717         -999    None   None    Blank
VAPOR_PRESS_770CM    .4592          1.9731         -999    None   None    Blank
VAPOR_PRESS_910CM    .6067          1.9161         -999    None   None    Blank
VAPOR_PRESS_ABV_CNPY .1338          2.3719         -999    None   None    None
SURF_PRESS           95.8           99.6           -999    None   None    Blank
DOWN_LONGWAVE_RAD_   155.5          421.12         -999    None   None    None
ABV_CNPY
UP_LONGWAVE_RAD_ABV_ 229.8          524.7          -999    None   None    None
CNPY
CORR_NET_RAD_ABV_    -95.01         788.3          -999    None   None    Blank
CNPY
ALBEDO               0              .965           -999    None   None    None
CNPY_AIR_TEMP_160CM  -4.114         31.87          -999    None   None    Blank
CNPY_WET_BULB_TEMP_  -4.17          19.32          -999    None   None    Blank
160CM
CNPY_VAPOR_PRESS_    .4415          2.0113         -999    None   None    Blank
160CM
MEAN_SMALL_TREE_     -24.48         39.03          -999    None   None    None
BIOMASS_TEMP
MEAN_MEDIUM_TREE_    -23.89         37             -999    None   None    None
BIOMASS_TEMP
MEAN_LARGE_TREE_     -21.88         35.56          -999    None   None    None
BIOMASS_TEMP
TOTAL_HEAT_STORAGE_  -146.1         102.7          -999    None   None    Blank
NORTH
TOTAL_HEAT_STORAGE_  -74.3          148.3          -999    None   None    Blank
WEST
MEAN_TOTAL_HEAT_     -62.1          89.2           -999    None   None    Blank
STORAGE
BIO_HEAT_STORAGE_    -12            9.2            -999    None   None    Blank
NORTH
BIO_HEAT_STORAGE_    -25.3          15             -999    None   None    Blank
WEST
MEAN_BIO_HEAT_       -10.5          6.2            -999    None   None    Blank
STORAGE
SENSIBLE_AIR_HEAT_   -44            22.6           -999    None   None    None
STORAGE
LATENT_AIR_HEAT_     -34.3          52.3           -999    None   None    None
STORAGE
SOIL_HEAT_STORAGE_   -66.7          46.8           -999    None   None    Blank
NORTH_10CM
SOIL_HEAT_STORAGE_   -89.8          76             -999    None   None    Blank
WEST_10CM
MEAN_SPECIFIC_HUM_   2.41           22.56          -999    None   None    Blank
ABV_CNPY
SDEV_SPECIFIC_HUM_   .012           10.84          -999    None   None    Blank
ABV_CNPY
MEAN_W_WIND_SPEED_   -1.997         1.979          -999    None   None    Blank
ABV_CNPY
SDEV_W_WIND_SPEED_   0              4.424          -999    None   None    Blank
ABV_CNPY
REL_HUM_ABV_CNPY     12.5           125.7          -999    None   None    Blank
CRTFCN_CODE          CPI            CPI            None    None   None    None
REVISION_DATE        15-JAN-1999    20-JAN-1999    None    None   None    None
--------------------------------------------------------------------------------

The following table gives information about the parameter values found in
the porometry data files.

                     Minimum        Maximum        Missng  Unrel  Below   Data
                     Data           Data           Data    Data   Detect  Not
Column Name          Value          Value          Value   Value  Limit   Cllctd
--------------------------------------------------------------------------------
SITE_NAME            NSA-YJP-FLXTR  NSA-YJP-FLXTR  None    None   None    None
SUB_SITE             9TF10-PR996    9TF10-PRWET    None    None   None    None
DATE_OBS             05-JUN-1994    07-OCT-1996    None    None   None    None
TIME_OBS             330            2330           None    None   None    None
TREE_HT_CLASS        <1.3           >1.3           None    None   None    None
MEASUREMENT_HT_CLASS <1.3           >1.3           None    None   None    None
STOMATAL_CONDUCT_H2O .0162          14.3745        -999    None   None    None
CRTFCN_CODE          CPI            CPI            None    None   None    None
REVISION_DATE        03-FEB-1999    03-FEB-1999    None    None   None    None
--------------------------------------------------------------------------------
Minimum Data Value -- The minimum value found in the column.
Maximum Data Value -- The maximum value found in the column.
Missng Data Value  -- The value that indicates missing data. This is used to
                      indicate that an attempt was made to determine the
                      parameter value, but the attempt was unsuccessful.
Unrel Data Value   -- The value that indicates unreliable data.  This is used
                      to indicate an attempt was made to determine the
                      parameter value, but the value was deemed to be
                      unreliable by the analysis personnel.
Below Detect Limit -- The value that indicates parameter values below the
                      instruments detection limits.  This is used to
                      indicate that an attempt was made to determine the
                      parameter value, but the analysis personnel determined
                      that the parameter value was below the detection
                      limit of the instrumentation.
Data Not Cllctd    -- This value indicates that no attempt was made to
                      determine the parameter value.  This usually
                      indicates that BORIS combined several similar but
                      not identical data sets into the same data base table
                      but this particular science team did not
                      measure that parameter.

Blank -- Indicates that blank spaces are used to denote that type of value.
N/A   -- Indicates that the value is not applicable to the respective column.
None  -- Indicates that no values of that sort were found in the column.
--------------------------------------------------------------------------------

7.4 Sample Data Record

Flux Data Record

SITE_NAME,SUB_SITE,DATE_OBS,TIME_OBS,SENSIBLE_HEAT_FLUX_ABV_CNPY,
LATENT_HEAT_FLUX_ABV_CNPY,NET_RAD_ABV_CNPY,CO2_FLUX_ABV_CNPY,CO2_CONC_ABV_CNPY,
CO2_STORAGE,CO2_FLUX_ABV_PLUS_STORAGE,NIGHT_CO2_FLUX_ABV_CNPY,DOWN_PPFD_ABV_CNPY,
UP_PPFD_ABV_CNPY,WIND_SPEED_510CM,WIND_SPEED_517CM,WIND_SPEED_610CM,
WIND_SPEED_710CM,WIND_SPEED_715CM,WIND_SPEED_770CM,WIND_SPEED_910CM,
WIND_SPEED_ABV_CNPY,MEAN_WIND_DIR_MAG_ABV_CNPY,SDEV_WIND_DIR_MAG_ABV_CNPY,
AIR_TEMP_ABV_CNPY,H2O_FLUX_ABV_CNPY,SOIL_HEAT_FLUX_NORTH_10CM,
SOIL_HEAT_FLUX_WEST_10CM,SOIL_TEMP_NORTH_1CM,SOIL_TEMP_NORTH_5CM,
SOIL_TEMP_NORTH_10CM,SOIL_TEMP_NORTH_25CM,SOIL_TEMP_NORTH_50CM,
SOIL_TEMP_NORTH_75CM,SOIL_TEMP_WEST_1CM,SOIL_TEMP_WEST_5CM,
SOIL_TEMP_WEST_10CM,SOIL_TEMP_WEST_25CM,SOIL_TEMP_WEST_50CM,
SOIL_TEMP_WEST_75CM,SOIL_TEMP_WEST_100CM,RAINFALL,DOWN_SOLAR_RAD_ABV_CNPY,
UP_SOLAR_RAD_ABV_CNPY,NET_SOLAR_RAD_ABV_CNPY,DOWN_TOTAL_RAD_ABV_CNPY,
UP_TOTAL_RAD_ABV_CNPY,AIR_TEMP_510CM,AIR_TEMP_517CM,AIR_TEMP_610CM,
AIR_TEMP_710CM,AIR_TEMP_715CM,AIR_TEMP_770CM,AIR_TEMP_910CM,
WET_BULB_TEMP_510CM,WET_BULB_TEMP_517CM,WET_BULB_TEMP_610CM,
WET_BULB_TEMP_710CM,WET_BULB_TEMP_715CM,WET_BULB_TEMP_770CM,
WET_BULB_TEMP_910CM,WET_BULB_TEMP_ABV_CNPY,VAPOR_PRESS_510CM,
VAPOR_PRESS_517CM,VAPOR_PRESS_610CM,VAPOR_PRESS_710CM,VAPOR_PRESS_715CM,
VAPOR_PRESS_770CM,VAPOR_PRESS_910CM,VAPOR_PRESS_ABV_CNPY,SURF_PRESS,
DOWN_LONGWAVE_RAD_ABV_CNPY,UP_LONGWAVE_RAD_ABV_CNPY,CORR_NET_RAD_ABV_CNPY,
ALBEDO,CNPY_AIR_TEMP_160CM,CNPY_WET_BULB_TEMP_160CM,CNPY_VAPOR_PRESS_160CM,
MEAN_SMALL_TREE_BIOMASS_TEMP,MEAN_MEDIUM_TREE_BIOMASS_TEMP,
MEAN_LARGE_TREE_BIOMASS_TEMP,TOTAL_HEAT_STORAGE_NORTH,TOTAL_HEAT_STORAGE_WEST,
MEAN_TOTAL_HEAT_STORAGE,BIO_HEAT_STORAGE_NORTH,BIO_HEAT_STORAGE_WEST,
MEAN_BIO_HEAT_STORAGE,SENSIBLE_AIR_HEAT_STORAGE,LATENT_AIR_HEAT_STORAGE,
SOIL_HEAT_STORAGE_NORTH_10CM,SOIL_HEAT_STORAGE_WEST_10CM,
MEAN_SPECIFIC_HUM_ABV_CNPY,SDEV_SPECIFIC_HUM_ABV_CNPY,
MEAN_W_WIND_SPEED_ABV_CNPY,SDEV_W_WIND_SPEED_ABV_CNPY,REL_HUM_ABV_CNPY,
CRTFCN_CODE,REVISION_DATE
'NSA-YJP-FLXTR','9TF10-FLX01',15-AUG-1993,630,-999.0,-999.0,-999.0,,,,,,-999.0,
-999.0,-999.0,,-999.0,-999.0,,,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,
-999.0,-999.0,-999.0,-999.0,-999.0,,,,-999.0,-999.0,-999.0,-999.0,-999.0,
-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,,-999.0,-999.0,
,,-999.0,-999.0,,-999.0,-999.0,,,-999.0,-999.0,-999.0,,-999.0,-999.0,,,-999.0,
-999.0,,-999.0,-999.0,,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,,,
-999.0,,,-999.0,-999.0,-999.0,,,,,,,,'CPI',15-JAN-1999
'NSA-YJP-FLXTR','9TF10-FLX01',15-AUG-1993,700,-999.0,-999.0,-999.0,,,,,,-999.0,
-999.0,-999.0,,-999.0,-999.0,,,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,
-999.0,-999.0,-999.0,-999.0,-999.0,,,,-999.0,-999.0,-999.0,-999.0,-999.0,
-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,,-999.0,-999.0,,,
-999.0,-999.0,,-999.0,-999.0,,,-999.0,-999.0,-999.0,,-999.0,-999.0,,,-999.0,
-999.0,,-999.0,-999.0,,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,-999.0,,,
-999.0,,,-999.0,-999.0,-999.0,,,,,,,,'CPI',15-JAN-1999



Porometry Data Record

SITE_NAME,SUB_SITE,DATE_OBS,TIME_OBS,TREE_HT_CLASS,MEASUREMENT_HT_CLASS,
STOMATAL_CONDUCT_H2O,CRTFCN_CODE,REVISION_DATE
'NSA-YJP-FLXTR','9TF10-PR996',08-JUL-1996,1530,'>1.3','>1.3',1.462,'CPI',03-FEB-1999
'NSA-YJP-FLXTR','9TF10-PR996',08-JUL-1996,1530,'>1.3','<1.3',1.843,'CPI',03-FEB-1999

